BEGIN_DESC
First test flight of the XL-70.  This is our XB-70 derived launch vehicle for the HyperDart.  We have made some modification to the orginal XB-70 design based on new materials and mission requirements.  The XB-70 is now capable of Mach 3.5+ with ease.  The XL can be a bit tricky to trim out since the engines are below the center of drag.  Trim will need constant attention based on throttle setting and altitude.
END_DESC

BEGIN_ENVIRONMENT
  System Sol
  Date MJD 57152.500000
END_ENVIRONMENT

BEGIN_FOCUS
  Ship XL70
END_FOCUS

BEGIN_CAMERA
  TARGET XL70
  MODE Extern
  POS 2.24 137.27 -0.15
  TRACKMODE TargetRelative
  FOV 40.00
END_CAMERA

BEGIN_HUD
  TYPE Surface
END_HUD

BEGIN_MFD Left
  TYPE Surface
  SPDMODE 1
END_MFD

BEGIN_MFD Right
  TYPE Orbit
  PROJ Ship
  FRAME Ecliptic
  ALT
  REF Earth
END_MFD

BEGIN_VC
END_VC


BEGIN_SHIPS
XL70:XL70
  STATUS Landed Earth
  POS -80.7092760 28.6261940
  HEADING 150.20
  PRPLEVEL 0:1.000
  NAVFREQ 0 0
  GEAR 1 1.0000
  WING 1 1.0000
  LIGHTS 0 1 1
  COG -2.000
  TEMP 284.206
END
ISS:ProjectAlpha_ISS
  STATUS Orbiting Earth
  RPOS 4108963.41 4867266.89 -2169906.11
  RVEL 5930.093 -4905.701 235.207
  AROT 110.01 -10.03 80.00
  PRPLEVEL 0:1.000
  IDS 0:588 10 1:586 10 2:584 10 3:582 10 4:580 10
  NAVFREQ 0 0
  XPDR 466
END
END_SHIPS

BEGIN_ExtMFD
END
